Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

BIOS API

All registers saved on entry and restores on return

BIOS Interrupts

Interrupt vector	Description	Version
10H	Video I/O	1+