Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

@PutChAtr

Brief

Print Char With Attribute

BIOS Interrupt

INT10H: H

Family API

fapi

Syntax

@PutChAtr char, atrib, page, repeat

Parameters

char (BYTE) - code of character

atrib (BYTE) - character attribute

col (BYTE) - column

row (BYTE) - row

page (BYTE) - optional video page number

Return